Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-12-89
P. 73

    UF4R10E0.book  Page 68  Tuesday, August 4, 2020  1:32 PM

                                                                           Care and storage

                                line, or any substance other  than a
                                rust inhibitor, into the air intake duct.
                                Do not spray flammable rust inhibitor
                                products on engine surfaces while the
                                engine is hot. Otherwise, a fire or ex-
                                plosion could occur. [EWJ02011]
                                                  1

                                                             2

                                 3           4
                              1 Breather hose
                              2 Clamp
                              3 Breather hose joint
                              4 Air intake duct
                            (6) Install the breather hose, and fasten the
                                breather hose with the clamp.
                            (7) Securely install the  hood in its original
                                position.

                                                                                                   68

| 68 69 70 71 72 73 74 75 76 77 78 |