Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - LIT-18626-12-89
P. 40

    UF4R10E0.book  Page 35  Tuesday, August 4, 2020  1:32 PM

                            Equipment operation

                            EJU37382                              EJU34882
                            Reboarding grip                       Stern eyes
                            The reboarding grip is used when boarding  The stern eyes are used to attach a rope to
                            the watercraft from the water.        the watercraft when transporting or mooring
                                                                  it.
                                      1

                                                                                                  1

                              1 Reboarding grip
                                                                   1 Stern eye
                            EJU34873
                            Bow eye
                                                                  EJU31677
                            The bow eye is used to attach a rope to the  Storage pouch
                            watercraft when transporting, mooring, or  The storage pouch is located on the bottom
                            towing it in an emergency. (See page 79 for  of the hood.
                            information on towing the watercraft.)  Use the  storage pouch to  store the own-
                                                                  er’s/operator’s manual and other small items.
                                                                  The storage pouch is not designed to be wa-
                                                                  terproof. If  you  carry objects  that must be
                                                                  kept dry, put them in a waterproof bag.
                                                                  To remove the storage pouch:
                                                                  (1) Remove the hood. (See page 33 for hood
                                                                     removal and installation procedures.)
                                 1
                                                                  (2) Unfasten  the bands, and  then remove
                                                                     the storage pouch.

                              1 Bow eye                                               2
                                                                                             1

                                                                   1 Storage pouch
                                                                   2 Band

                            35

| 35 36 37 38 39 40 41 42 43 44 45 |