Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 90 - LIT-18626-12-90
P. 90

    UF4P10E0.book  Page 84  Friday, July 31, 2020  8:50 AM

                            Operation

                            (3) Have the first passenger move to the rear  (6) Make sure that  the passenger(s)  have
                                of the watercraft.                   their feet on the floor of the footwell and
                                                                     are securely holding on to the person in
                                                                     front of them or to the handgrip provided.

                            (4) Have the first passenger board using the
                                same procedure as the operator, place
                                their feet on the floor of the footwell, and  (7) Attach the engine shut-off cord (lanyard)
                                securely hold on to the operator.    to your left wrist, and then attach the clip
                                                                     to the engine shut-off switch.
                                                                  (8) Look  in all directions, start  the  engine,
                                                                     and then start off slowly.
                                                                  EJU33084
                                                                  Starting off
                                                                  EWJ00713

                                                                  To avoid collisions:
                                                                   Scan constantly for people, objects, and
                                                                   other watercraft. Be alert for conditions
                                                                   that limit your visibility or block your vi-
                            (5) Have the second passenger  follow the
                                                                   sion of others.
                                same procedure. When the second pas-
                                                                   Operate defensively at safe speeds and
                                senger is boarding,  try to  balance the
                                                                   keep a safe distance away from people,
                                watercraft together with the first passen-
                                                                   objects, and other watercraft.
                                ger.
                                                                   Do not follow directly behind watercraft
                                                                   or other boats. Do not go near others to
                                                                   spray or splash them with water, go too
                                                                   close to other boats, or go too fast for
                                                                   the traffic conditions. Avoid sharp turns
                                                                   or other maneuvers that make it hard for
                                                                   others to avoid you or understand where
                                                                   you are going.  Avoid areas with sub-
                                                                   merged objects or shallow water.
                                                                   Take early action to avoid collisions. Re-
                                                                   member, watercraft and other boats do

                            84

| 85 86 87 88 89 90 91 92 93 94 95 |