Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-90
P. 44

    UF4P10E0.book  Page 38  Friday, July 31, 2020  8:50 AM

                            Watercraft operation

                                angle can be adjusted in the range of the  Vertical movement of the bow will be reduced
                                trim settings –2 to +2.           and the watercraft will get up on plane more
                                                                  quickly when accelerating.

                                       1

                              1 “TRIM/T.D.E.” switch
                            Bow-up positions
                            The bow will go up, causing the trim angle to
                            increase.
                            There is less water resistance, therefore,
                            straight-ahead acceleration is enhanced.

                            Bow-down positions
                            The bow will go down, causing the trim angle
                            to decrease.

                            38

| 39 40 41 42 43 44 45 46 47 48 49 |