Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-12-92
P. 59

    UF4S10E0.book  Page 53  Monday, September 28, 2020  1:50 PM

                                                                     Equipment operation

                            when released. WARNING! Do not use the  EJU34873
                                                                  Bow eye
                            reboarding step to lift the watercraft. The
                                                                  The bow eye is used to attach a rope to the
                            reboarding step is not designed to support
                                                                  watercraft  when transporting, mooring, or
                            the watercraft’s weight. If the reboarding
                                                                  towing it in an emergency. (See page 103 for
                            step  breaks,  the watercraft could fall,
                                                                  information on towing the watercraft.)
                            which could result in severe injury. [EWJ01212]

                                                     1

                                                                     1
                                                                   1 Bow eye
                              1 Reboarding step                   EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                                                                  it.

                            ECJ00743                                               1

                            Use the reboarding step only to board the
                            watercraft in the water. Do not use the re-  1 Stern eye
                            boarding step for any other purpose. The  EJU40423
                            watercraft can be damaged.            Cleat
                                                                  The cleat is used to attach a ski rope to the
                                                                  watercraft  when pulling a wakeboarder or
                                                                  water-skier.  WARNING! Do not use the
                                                                  cleat to lift the watercraft. The cleat is not
                                                                  designed to support the watercraft’s
                                                                  weight. If the cleat breaks, the watercraft

                                                                                                   53

| 54 55 56 57 58 59 60 61 62 63 64 |