Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-92
P. 50

    UF4S10E0.book  Page 44  Monday, September 28, 2020  1:50 PM

                            Instrument operation

                            TIP:                                  TIP:
                            The accuracy of the fuel level meter varies   The display units of the speedometer are
                            depending on the operating conditions. Use  selected according to the display units of
                            this function as a reference only.     the multifunction information center. (See
                            EJU45151                               page 45 for information on  switching  the
                            Home screen “ ”
                                                                   display units.)
                            The center display of the home screen shows
                                                                   When operating the watercraft in reverse,
                            the speedometer and the indicators for the
                                                                   or when moving forward or in reverse at a
                            operation modes. (See page 36 for informa-
                                                                   very low speed using the T.D.E., “0” will be
                            tion on the functions of the various modes.)
                                                                   displayed on the speedometer.
                            TIP:                                  EJU45970
                                                                  Information screen “  ”
                            If the engine speed increases while the drive
                                                                  The information screens show the trip infor-
                            control mode screen, setting menu screen, or
                                                                  mation and fuel information in the center dis-
                            engine lock screen  is  displayed, the  multi-
                                                                  play.
                            function information center will automatically
                            switch to the home screen.            TIP:
                                                                  The display units for the distances and fuel
                                             1
                                                                  amounts are selected according to the dis-
                                                                  play units of the  multifunction  information
                                                                  center. (See page 45 for information on
                                                     MPH
                                                                  switching the display units.)
                                                     RPM
                                                                               Trip/Fuel Info
                              2   Reverse Assist  +2              1      0.7 Trip Hrs.  1.6 Av MPG  4
                              3   T.D.E. FORWARD                  2      0.6 Trip Miles  0.3 Gal used  5
                              4   No Wake  +1                     3      0.9 Engine Hrs.  0.6 GpH  6
                              5   Cruise Assist  +4                              Reset All

                              6   Drive Control                                    7
                                                                   1 Trip time
                              1 Speedometer                        2 Distance traveled
                              2 Reverse assist indicator           3 Total engine hours
                              3 T.D.E. indicator                   4 Average fuel consumption per gallon or liter
                              4 No-wake mode indicator             5 Total fuel used
                              5 Cruise assist indicator            6 Fuel consumption per hour
                              6 Drive control indicator            7 “Reset All”
                            Speedometer
                            The speedometer shows the watercraft
                            speed.

                            44

| 45 46 47 48 49 50 51 52 53 54 55 |