Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-12-92
P. 97

    UF4S10E0.book  Page 91  Monday, September 28, 2020  1:50 PM

                                                                           Care and storage

                             Steering cable (jet thrust nozzle end)

                             Shift rod (reverse gate end) and ball joint

                            TIP:
                            Disconnect the shift rod from the ball joint be-
                            fore lubricating.
                            EJU40263
                            Rustproofing
                            Spray metallic parts of the hull, deck, and en-
                            gine with a rust inhibitor such as Yamalube
                            Silicone Protectant & Lubricant.
                            Have a Yamaha dealer rustproof the internal
                            engine components.

                                                                                                   91

| 92 93 94 95 96 97 98 99 100 101 102 |