Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-93
P. 69

    UF4N10E0.book  Page 62  Tuesday, September 29, 2020  8:02 AM

                                                                     Equipment operation

                            returns automatically to its original position  ECJ00743
                            when released. WARNING! Do not use the
                            reboarding step to lift the watercraft. The  Use the reboarding step only to board the
                            reboarding step is not designed to support  watercraft in the water. Do not use the re-
                            the watercraft’s weight. If the reboarding  boarding step for any other purpose. The
                            step  breaks,  the watercraft could fall,  watercraft can be damaged.
                            which could result in severe injury. [EWJ01212]
                                                                  EJU34873
                            VX / VX DELUXE                        Bow eye
                                                                  The bow eye is used to attach a rope to the
                                                                  watercraft  when transporting, mooring, or
                                                     1
                                                                  towing it in an emergency. (See page 115 for
                                                                  information on towing the watercraft.)

                              1 Reboarding step
                            VX CRUISER / VX LIMITED
                                                                     1
                                                     1
                                                                   1 Bow eye
                                                                  EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                                                                  it.

                              1 Reboarding step

                                                                                   1

                                                                   1 Stern eye

                                                                                                   62

| 64 65 66 67 68 69 70 71 72 73 74 |