Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 119 - LIT-18626-12-93
P. 119

    UF4N10E0.book  Page 112  Tuesday, September 29, 2020  8:02 AM

                                                                           Trouble recovery

                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Watercraft slow or   Watercraft op-  Drive control mode   Deactivate or adjust
                             loses power      eration mode   activated    drive control mode
                                              (VX DELUXE /                                     42
                                              VX CRUISER /
                                              VX LIMITED)
                                              Cavitation  Jet intake clogged  Clean           113
                                                         Impeller damaged or   Have serviced by   113
                                                         worn             Yamaha dealer
                                              Engine over-  Engine speed reduc-  Clean jet intake and   49, 56
                                              heat warning  tion control activated  cool engine
                                              Oil pressure   Engine speed reduc-  Add oil    48, 57
                                              warning    tion control activated
                                              Spark plug  Fouled or defective  Have serviced by   —
                                                                          Yamaha dealer
                                                         Incorrect heat range  Have serviced by   —
                                                                          Yamaha dealer
                                                         Gap incorrect    Have serviced by     —
                                                                          Yamaha dealer
                                              Electrical wir-  Loose connection  Have serviced by   —
                                              ing                         Yamaha dealer
                                              Fuel       Stale or contaminat-  Have serviced by   —
                                                         ed               Yamaha dealer
                                              Air filter  Clogged         Have serviced by     —
                                                                          Yamaha dealer
                                                         Oil buildup      Have serviced by     —
                                                                          Yamaha dealer
                                              Throttle lever  Faulty      Have serviced by     —
                                                                          Yamaha dealer
                             Audio system does   Fuse    Burned out       Have serviced by
                             not activate                                 Yamaha dealer        —
                             (equipped models)

                                                                                                 112

| 114 115 116 117 118 119 120 121 122 123 124 |