Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-12-93
P. 70

    UF4N10E0.book  Page 63  Tuesday, September 29, 2020  8:02 AM

                            Equipment operation

                            EJU40423                              cleats break, the watercraft could fall,
                            Cleat
                                                                  which could result in severe injury. [EWJ00822]
                            The cleat is used to attach a ski rope to the
                            watercraft  when pulling a  wakeboarder or
                            water-skier.  WARNING!  Do not use the                              1
                            cleat to lift the watercraft. The cleat is not
                            designed to support the watercraft’s             2
                            weight. If the cleat breaks, the watercraft
                            could fall, which could result in severe in-
                            jury. [EWJ01511]

                                                         1
                                                                   1 Pull-up cleat (VX CRUISER / VX LIMITED)
                                                                   2 Pull-up cleat (VX LIMITED)
                                                                  EJU31685
                                                                  Storage compartments
                                                                  This watercraft is equipped with the following
                                                                  storage compartments.
                                                                  The storage compartments are not designed
                              1 Cleat                             to be waterproof.  If you carry objects that
                                                                  must be kept dry, put them in a waterproof
                            EJU34894
                            Pull-up cleats (VX CRUISER / VX       bag.
                            LIMITED)                              Make sure  that the storage  compartments
                            The pull-up cleats are used to attach a rope  are closed securely before operating the wa-
                            to the watercraft when mooring it.    tercraft.
                            To use a pull-up cleat, pull it up. The pull-up  EJU45250
                            cleat returns automatically to its original posi-  Bow storage compartment
                                                                  The bow storage compartment is located un-
                            tion when released. WARNING! Do not use
                                                                  der the hood.
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                            the watercraft’s weight. If the pull-up

                            63

| 65 66 67 68 69 70 71 72 73 74 75 |