Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 99 - LIT-18626-13-05
P. 99

    UF4P11E0.book  Page 93  Friday, October 30, 2020  9:39 AM

                                                                           Care and storage

                             Steering cable (jet thrust nozzle end), elec-
                              tric trim rod (jet thrust nozzle end), and ball
                              joint

                            TIP:
                            Disconnect the electric trim rod from the ball
                            joint before lubricating.
                             Shift rod (reverse gate end) and ball joint

                            TIP:
                            Disconnect the shift rod from the ball joint be-
                            fore lubricating.
                            EJU40263
                            Rustproofing
                            Spray metallic parts of the hull, deck, and en-
                            gine with a rust inhibitor such as Yamalube
                            Silicone Protectant & Lubricant.
                            Have a Yamaha dealer rustproof the internal
                            engine components.

                                                                                                   93

| 94 95 96 97 98 99 100 101 102 103 104 |